ATLAS SCIENTIFIC PH SENSOR:

VCC OF CARIIER BOARD TO 5V OF RASPI

TX OF CARIIER BOARD TO GPIO2 SDA

RX OF CARIIER BOARD TO GPIO 3 SCL

sudo apt-get update

sudo apt-get upgrade

git clone <https://github.com/AtlasScientific/Raspberry-Pi-sample-code.git>

sudo nano /boot/cmdline.txt

delete the command: console=serial0,115200

sudo pip install pyserial

cd ~/Raspberry-Pi-sample-code

sudo python uart.py